* CRT stands for Cathode Ray Tube and LCD stands for Liquid Crystal Display
* The screen size is measured diagonally
* Active-matrix LCDs use the TFT-Technology
* The unit which is used to measure the brightness of a display is called cd/m^2 (candela per square meter)
* In a CRT monitor phosphor is used to produce light
* The three advantages of a OLED display are: They use less energy, the produce brighter colors and they are flexible